**ChemoSHIELD®**

**Model: CS500**

|  |  |
| --- | --- |
| **Electrical** | |
|  | Total Amps: 12 Amps: 1.5 Volts: 115 Watts: 175 BTU/HR: 580 |
| **Classification** | |
|  | NSF Listed: n/a NSF Class: n/a NSF Type: n/a Old NSF Class: n/a Old NSF Type: n/a |
| **Weight** | |
|  | Net Weight: 570 Ship Weight: 660 |
| **Containment** | |
|  | Particulates: particulates (PPE) Vapors and Gases: particulates (PPE), vapor (PPE if exhausted, treat |
| **Performance** | |
|  | Face Velocity: n/a Recirculated Air %: 0 Exhausted Air %: 100% |
| **Exhaust** | |
|  | Contaminated Pressure Plenum: Negative Exhaust Source: External Exhaus Exhaust Destination: Outdoors Exhaust Connection: Hard Exhaust CFM: 310 Inches Of Water (Column): -1.8 |
| **Filter** | |
|  | HEPA Supply Filter(s): yes HEPA Exhaust Filter: yes |
| **Features** | |
|  | StediVOLT: n/a, outlets GF UniPressure: no Stand: Standard Warranty: 36 months (USA only); 12 months (international) |