**ChemoSHIELD®**

**Model: CS500**

|  |
| --- |
| **Electrical** |
|   | Total Amps: 12Amps: 1.5Volts: 115Watts: 175BTU/HR: 580 |
| **Classification** |
|   | NSF Listed: n/aNSF Class: n/aNSF Type: n/aOld NSF Class: n/aOld NSF Type: n/a |
| **Weight** |
|   | Net Weight: 570Ship Weight: 660 |
| **Containment** |
|   | Particulates: particulates (PPE)Vapors and Gases: particulates (PPE), vapor (PPE if exhausted, treat |
| **Performance** |
|   | Face Velocity: n/aRecirculated Air %: 0Exhausted Air %: 100% |
| **Exhaust** |
|   | Contaminated Pressure Plenum: NegativeExhaust Source: External ExhausExhaust Destination: OutdoorsExhaust Connection: HardExhaust CFM: 310Inches Of Water (Column): -1.8 |
| **Filter** |
|   | HEPA Supply Filter(s): yesHEPA Exhaust Filter: yes |
| **Features** |
|   | StediVOLT: n/a, outlets GFUniPressure: noStand: StandardWarranty: 36 months (USA only); 12 months (international) |